IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2020-04-10T22:45:57"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190508_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "vbu737AR" of Organization (no name given)
  Owner history of Person "vbu737AR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "09479279 Cover part for urinal flusher, 6 V, Bluetooth" | object type "09479279 Cover part for urinal flusher, 6 V, Bluetooth" | names: "09479279:09479279 Cover part for urinal flusher, 6 V, Bluetooth:377719" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Other

Types
  IFCVALVETYPE "09479279 Cover part for urinal flusher, 6 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions(Type), Electrical(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "09479279" (IFCTEXT)
    Features = "Trim Kit;Touchless;Bluetooth®;Battery-operated" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "09479279" (IFCTEXT)
    Name = "09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "12 x 140 x 140 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/09479279" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/09479279" (IFCTEXT)
    Class = "Trim Kit;Touchless;Bluetooth®;Battery-operated" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/09479279" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/09479279/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/09479279" (IFCTEXT)
    Group = "Urinals" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "BEL;CZE;DEU;ESP;FRA;INT;ITA;NLD;SVK" (IFCTEXT)
    Model = "09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCTEXT)
    Name_en = "09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "0.87 kg" (IFCTEXT)
    Package external Dimensions = "210 x 165 x 60" (IFCTEXT)
    Product Code = "09479279" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/09479279/en" (IFCTEXT)
    Product Family = "HANSAELECTRA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/09479279" (IFCTEXT)
    Product URL = "http://static.hansa.com/09479279" (IFCTEXT)
    Type Name = "09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "HANSA" (IFCLABEL)
    ModelReference = "09479279" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 500. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0228745230645791 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000229216614520563 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "25" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "09479279: 09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCLABEL)
    Family and Type = "09479279: 09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "09479279: 09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCLABEL)
    Type Id = "09479279: 09479279 Cover part for urinal flusher, 6 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 11.7 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 140. (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Battery = "Lithium 2CR5 6 V" (IFCTEXT)
    Bluetooth = "4.x" (IFCTEXT)
    Electrical Connection = "n/a" (IFCTEXT)
    Operating Voltage = 6. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55" (IFCTEXT)
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "09479279" (IFCTEXT)
    ConvergoRefNr = "0087-2003-0057-FI" (IFCTEXT)
    ManufacterURL = "http://www.hansa.com/" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    NBSDescription = "Urinal flushing valves" (IFCTEXT)
    NBSReference = "45-35-70/355" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_35_93_80" (IFCTEXT)
    Uniclass2015Description = "Urinal flushing valves" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_93_79" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "02/04/2020" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Customs Code = "84819000" (IFCTEXT)
    EAN Number = "4057304014048" (IFCTEXT)
    EMC Directive = "2014/30/EU" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "Twist-resistant;Adjustable settings (via bluetooth)" (IFCTEXT)
    Afterflush Period = "6 s (1-20 s)" (IFCTEXT)
    Automatic Flush = "24 h (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "6 s (1-120 s)" (IFCTEXT)
    Electronic Parts = "Autofocus sensor;Solenoid valve;Low battery indication" (IFCTEXT)
    Flow Rate At 300kPa = 0.00706293334429772 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Included = "Square rosette" (IFCTEXT)
    Installation Type = "Wall mounted for concealed unit" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/09479279" (IFCTEXT)
    Max. Hot Water Supply = 70. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Pre-flush Period = "2 s (OFF / 1-10 s)" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/09479279" (IFCTEXT)