IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-06-23T19:31:03"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Alternate UI 20.2.12.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1687537861 (2023-06-23T16:31:01Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "48372331 Bath and shower faucet with shower set" | object type "48372331(2023):48372331 Bath and shower faucet with shower set" | names: "48372331(2023):48372331 Bath and shower faucet with shower set:24221" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "48372331 Bath and shower faucet with shower set" | FAUCET | 1 occurrence | material: "Brass" | property sets: Constraints, Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetDefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Hand Shower Visibility = TRUE (IFCBOOLEAN)
    HandShowerDefaultElevation = 1200. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.484405229450147 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.033203636905191 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    FaucetNominalDepth = 188.369187497352 (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalHeight = 73.1867716110686 (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalWidth = 342.419846372953 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalDepth = 124.155619664545 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalHeight = 969.556135673181 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalWidth = 236.514413633324 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "9" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/48372331" (IFCTEXT)
    3D View = "https://static.hansa.com/AR/48372331" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/48372331" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/48372331" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/48372331/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/48372331" (IFCTEXT)
    Group = "Bath and shower faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/48372331" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/48372331" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "Austria;Belgium;Czech Republic;Germany;Spain;France;International;Italy;Netherlands;Slovakia" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/48372331" (IFCTEXT)
    Model = "48372331 Bath and shower faucet with shower set" (IFCTEXT)
    Name_en = "48372331 Bath and shower faucet with shower set" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "48372331" (IFCTEXT)
    Product Family = "HANSAOPTIMA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/48372331" (IFCTEXT)
    Product URL = "http://static.hansa.com/48372331" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/48372331/en" (IFCTEXT)
    Type Name = "48372331 Bath and shower faucet with shower set" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Flexible length / can be shortened;Hose guide, revolving" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Connection = "Eccentric coupling(s);Cover plate(s);Silencer(s)" (IFCTEXT)
    Connection Size = "G3/4" (IFCTEXT)
    Diverter = "Turn operated diverter;Integrated into flow control handle" (IFCTEXT)
    Eco Flow At 300kPa = 0.00423776000657863 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Rate At 300kPa = 0.00776922667872749 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower Size = "Ø110" (IFCTEXT)
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation Width = "CC150± 15 mm" (IFCTEXT)
    Lever Handle = "Temperature control handle;Flow control handle;Hot/Cold symbols;Easy-Grip surface;Eco feature for water flow" (IFCTEXT)
    Max. Hot Water Supply = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part for flow control;Thermostatic cartridge for automatic temperature control;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Mounting Holes = "2 hole" (IFCTEXT)
    Pressure Loss With Flow 02ls = 250000. (IFCPRESSUREMEASURE) [PASCAL]
    Shower Parts = "Hand shower;;Adjustable shower rail bracket;Shower hose (1750 mm);Shower rail;Anti limescale technology (easy to clean);Soap dish;Twist guard for shower hose;Variable fixing points" (IFCTEXT)
    Shower Spray = "Normal;Massage;Rain" (IFCTEXT)
    Shower Spray Number = "3 shower sprays" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature = "Temperature limiter (retrofittable);Thermostatic safety stop at 38°C" (IFCTEXT)
    Temperature Adjustments = "Safety stop against scalding at 38°C;The housing of the fittings conducts minimal heat" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "48372331(2023): 48372331 Bath and shower faucet with shower set" (IFCLABEL)
    Family and Type = "48372331(2023): 48372331 Bath and shower faucet with shower set" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "48372331(2023): 48372331 Bath and shower faucet with shower set" (IFCLABEL)
    Type Id = "48372331(2023): 48372331 Bath and shower faucet with shower set" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "48372331(2023)" (IFCTEXT)
    Features = "Thermostatic" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass/Plastic" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "48372331" (IFCTEXT)
    Name = "48372331 Bath and shower faucet with shower set" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "Faucet: 345x190x75 mm ; Shower: 235x125x970 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "48372331(2023)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Shower mixers" (IFCTEXT)
    NBSReference = "45-35-70/335" (IFCTEXT)
    ProductInformation = "Thermostatic shower faucet with spout" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_81" (IFCTEXT)
    Uniclass2015Description = "Shower thermostatic water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_81" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/06/2023" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4057304018190" (IFCTEXT)
    EN Standard = "EN1111" (IFCTEXT)
    ETIM Class Number = "EC010862 Bath mixing tap" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "981 x 241 x 79" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.hansa.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.hansa.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/48372331" (IFCTEXT)
    URL Declaration of SCIP = "http://static.hansa.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.hansa.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.hansa.com/doc/EcoLabel" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL UWL = "http://static.hansa.com/UWL/48372331" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)