IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2024-04-26T18:51:47"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Alternate UI 20.2.12.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1714146707 (2024-04-26T15:51:47Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "88619085 Cover part for shower faucet" | object type "88619085:88619085 Cover part for shower faucet" | names: "88619085:88619085 Cover part for shower faucet:13189" | property sets: Constraints, Dimensions, Identity Data, Other, Phasing

Types
  IFCVALVETYPE "88619085 Cover part for shower faucet" | FAUCET | 1 occurrence | property sets: Constraints, Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0531166571246554 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00205904912375712 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    NominalDepth = 71.2790171155186 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 169.981381941885 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 169.999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/88619085" (IFCTEXT)
    3D View = "https://static.hansa.com/AR/88619085" (IFCTEXT)
    Ambience photo = "http://static.hansa.com/ambience/88619085" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/88619085" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/88619085" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/88619085/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/88619085" (IFCTEXT)
    Group = "Shower faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/88619085" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/88619085" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Switzerland;Belgium;Netherlands;France;Czech Republic;Slovakia;Hungary;Romania;Italy;Spain;Greece;Portugal;Australia" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/88619085" (IFCTEXT)
    Model = "88619085 Cover part for shower faucet" (IFCTEXT)
    Name_en = "88619085 Cover part for shower faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "88619085" (IFCTEXT)
    Product Family = "HANSACLINICA Safety+" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/88619085" (IFCTEXT)
    Product URL = "http://static.hansa.com/88619085" (IFCTEXT)
    Spare-Part Information URL = "http://static.hansa.com/sp/88619085" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/88619085/en" (IFCTEXT)
    Type Name = "88619085 Cover part for shower faucet" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "88619085: 88619085 Cover part for shower faucet" (IFCLABEL)
    Family and Type = "88619085: 88619085 Cover part for shower faucet" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "88619085: 88619085 Cover part for shower faucet" (IFCLABEL)
    Type Id = "88619085: 88619085 Cover part for shower faucet" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "88619085" (IFCTEXT)
    Features = "Trim Kit;Thermostatic" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "88619085" (IFCTEXT)
    Name = "88619085 Cover part for shower faucet" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "170x70x170 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "88619085" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Shower mixers" (IFCTEXT)
    NBSReference = "45-35-70/335" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "20/04/2024" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Approval ABP = "PA-IX 38187/IC" (IFCTEXT)
    Approval DVGW = "DW-6509CS0197" (IFCTEXT)
    CO2 Emissions (A1-A3) = 26.92 (IFCREAL)
    CO2 Emissions (A4) = 0.44 (IFCREAL)
    CO2 Emissions (B7) = 4400.4 (IFCREAL)
    CO2 Emissions (C2) = 0.02 (IFCREAL)
    CO2 Emissions (C3) = 0.02 (IFCREAL)
    CO2 Emissions (C4) = 0.35 (IFCREAL)
    CO2 Emissions (D) = -8.33 (IFCREAL)
    EAN Number = "4057304012532" (IFCTEXT)
    EN Standard = "EN 1111" (IFCTEXT)
    ETIM Class Number = "EC010546 Mechanical control system for shower" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "204 x 186 x 174" (IFCTEXT)
    UNSPSC Class Number = "30181810 Faucet trim" (IFCTEXT)
    URL ABP = "http://static.hansa.com/ABP/88619085" (IFCTEXT)
    URL DVGW = "http://static.hansa.com/DVGW/88619085" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.hansa.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.hansa.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/88619085" (IFCTEXT)
    URL Declaration of SCIP = "http://static.hansa.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.hansa.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.hansa.com/doc/EcoLabel" (IFCTEXT)
    URL Environmental Product Declaration EPD = "http://www.hansa.com/fileadmin/resources/182036_Oras Group EPD_Cover part for bath and shower faucet.pdf" (IFCTEXT)
    URL Materials Declaration = "http://www.hansa.com/fileadmin/resources/169384_88619085_materialsdeclaration.pdf" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Chrome" (IFCLABEL)
  Mechanical | properties | on 1 type object
    Additional Features = "protected against back-flow in domestic use (according to DIN EN 1717) Safety lock against scalding 38°C (36°-44°)" (IFCTEXT)
    Advanced Features = "Thermal disinfection without cartridge readjustment" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Concealed Parts = "Round rosette;Function unit;BLUECLICK for an easy, screwless trim plate installation;BLUETUNE alignment after installation of +/- 3,5º" (IFCTEXT)
    DN Size = "170 mm" (IFCTEXT)
    Flow Rate At 300kPa = 0.0134195733541657 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Concealed wall mounting" (IFCTEXT)
    Lever Handle = "Temperature control handle;Flow control handle" (IFCTEXT)
    Max. Hot Water Supply = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part for flow control;Thermostatic cartridge for automatic temperature control;Non-return valve(s)" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature = "" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)

Other addresses and roles
  2 x postal address (none given)