IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2018-08-20T16:36:42"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.0.490.0 - Alternate UI 16.6.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "cjl@convergo.se" of Organization (no name given)
  Owner history of Person "cjl@convergo.se" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "09450170 Body for urinal flusher" | object type "09450170 Body for urinal flusher" | names: "09450170:09450170 Body for urinal flusher:330191" | material: materials ("Plastic, Opaque Black", "Brass") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "09450170 Body for urinal flusher" | FAUCET | 1 occurrence | material: materials ("Plastic, Opaque Black", "Brass") | property sets: Dimensions, Electrical, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "09450170: 09450170 Body for urinal flusher" (IFCLABEL)
    Family and Type = "09450170: 09450170 Body for urinal flusher" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "09450170: 09450170 Body for urinal flusher" (IFCLABEL)
    Type Id = "09450170: 09450170 Body for urinal flusher" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Public & semi-public" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "09450170" (IFCTEXT)
    Features = "Concealed" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "09450170" (IFCTEXT)
    Name = "09450170 Body for urinal flusher" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "185x102x247 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Group = "Installation Technology" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Market = "BEL;CHE;CZE;DEU;ESP;FRA;INT;ITA;NLD;PRT" (IFCTEXT)
    Model = "09450170 Body for urinal flusher" (IFCTEXT)
    Name_en = "09450170 Body for urinal flusher" (IFCTEXT)
    OmniClass Number = "23.45.55.11" (IFCTEXT)
    OmniClass Title = "Sanitary Components" (IFCTEXT)
    Product Code = "09450170" (IFCTEXT)
    Product Datasheet = "http://dbint.hansa.com/index.php?pdf=true&pdfType=prod&catType=p" (IFCTEXT)
    Product Family = "HANSAELECTRA" (IFCTEXT)
    Product URL = "http://dbint.hansa.com/index.php?IdProduct=88411&IdTreeGroup=2320" (IFCTEXT)
    Type Name = "09450170 Body for urinal flusher" (IFCTEXT)
    URL = "" (IFCTEXT)
    Usage Group = "Hospitals" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "09450170" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "09450170 Body for urinal flusher" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    NotTrimKitVisibility = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    TrimKitVisibility = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.155575561035895 (IFCAREAMEASURE) [SQUARE_METRE]
    NominalDepth = 102. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00466031183109498 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 247. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 185. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Sanitary" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Installation Type = "Wall mounted concealed" (IFCTEXT)
    Installation and Maintenance = "http://dbint.hansa.com/media/hansa_sanitaer/bedienungsanleitungen/print/aktuell/0750/M09450170_a.pdf" (IFCTEXT)
    Mechanical Parts = "Litter filter(s)" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBSSpecificationPath = "" (IFCTEXT)
  General | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "09450170" (IFCTEXT)
    ConvergoRefNr = "0087-1809-0026-FI" (IFCTEXT)
    ManufacterURL = "http://www.hansa.com/" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_65_52_61_15" (IFCTEXT)
    Uniclass2015Description = "Concealed intumescent pipe collars" (IFCTEXT)
    Uniclass2015Reference = "Pr_65_52_61_15" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "08/08/2018" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Electrical | properties | on 1 type object
    Electronic Parts = "Solenoid valve" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4015474277373" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    BaseunitMainMaterial = "Brass" (IFCLABEL)