IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2020-04-10T22:42:05"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190508_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "vbu737AR" of Organization (no name given)
  Owner history of Person "vbu737AR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "06142209 Washbasin faucet, 9/12 V, Bluetooth" | object type "06142209 Washbasin faucet, 9/12 V, Bluetooth" | names: "06142209:06142209 Washbasin faucet, 9/12 V, Bluetooth:362789" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "06142209 Washbasin faucet, 9/12 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions(Type), Electrical(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Bathroom;Public & Semi-public" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "Single lever" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "06142209" (IFCTEXT)
    Features = "Touchless;Bluetooth®;Plug transformer" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "06142209" (IFCTEXT)
    Name = "06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "65x155x130 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/06142209" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/06142209" (IFCTEXT)
    Class = "Touchless;Bluetooth®;Plug transformer" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/06142209" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/06142209/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/06142209" (IFCTEXT)
    Group = "Washbasin Faucets" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Market = "AUT;BEL;CZE;DEU;ESP;FRA;INT;ITA;NLD;SVK" (IFCTEXT)
    Model = "06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCTEXT)
    Name_en = "06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "2.071 kg" (IFCTEXT)
    Package external Dimensions = "290 x 210 x 90" (IFCTEXT)
    Product Code = "06142209" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/06142209/en" (IFCTEXT)
    Product Family = "HANSALIGNA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/06142209" (IFCTEXT)
    Product URL = "http://static.hansa.com/06142209" (IFCTEXT)
    Type Name = "06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "06142209" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0396551751230666 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00131774053782049 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "20" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "06142209: 06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCLABEL)
    Family and Type = "06142209: 06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "06142209: 06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCLABEL)
    Type Id = "06142209: 06142209 Washbasin faucet, 9/12 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 155.223165740614 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 127.600000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 66.2928819806354 (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 110. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Bluetooth = "4.x" (IFCTEXT)
    Electrical Connection = "230 / 9 V" (IFCTEXT)
    Operating Voltage = 12. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55 / transformer IP 20" (IFCTEXT)
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "06142209" (IFCTEXT)
    ConvergoRefNr = "0087-2003-0037-FI" (IFCTEXT)
    ManufacterURL = "http://www.hansa.com/" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "06/04/2020" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "4057304014161" (IFCTEXT)
    EMC Directive = "2014/30/EU" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "Adjustable settings (via bluetooth)" (IFCTEXT)
    Aerator = "HONEYCOMB®" (IFCTEXT)
    Afterflow Period = 3. (IFCREAL)
    Automatic Flush = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Connection = "Flexible Inlet Pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    DN Size = "DN15" (IFCTEXT)
    Electronic Parts = "Autofocus sensor;Solenoid valve;" (IFCTEXT)
    Extensions = "Rapid pop-up waste" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.00353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/06142209" (IFCTEXT)
    Lever Handle = "Temperature control handle" (IFCTEXT)
    Max Flow Period = 120. (IFCREAL)
    Max. Hot Water Supply = 70. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Mixing valve;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Mounting Holes = "1 Mounting Hole" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/06142209" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Temperature = "Temperature limiter (retrofittable)" (IFCTEXT)