IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-06-23T19:38:37"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Alternate UI 20.2.12.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1687538317 (2023-06-23T16:38:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "45252219 Washbasin faucet, 3 V, Bluetooth" | object type "45252219(2023):45252219 Washbasin faucet, 3 V, Bluetooth" | names: "45252219(2023):45252219 Washbasin faucet, 3 V, Bluetooth:38516" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "45252219 Washbasin faucet, 3 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Constraints, Dimensions, Electrical, General, Green Building Properties, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0465121680761151 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00143256628112184 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 166.628893602525 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 171.000000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 50.1115016040878 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "15" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/45252219" (IFCTEXT)
    3D View = "https://static.hansa.com/AR/45252219" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/45252219" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/45252219" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/45252219/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/45252219" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/45252219" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/45252219" (IFCTEXT)
    Long Marketing = "Clinica Hybrid series is giving you a whole new modern design to fit into any bathroom. The long loop lever gives you easy and intuitive operation and with our intelligent touchless functions build into same faucet it also supports hygiene operation without any touch needed. Key Features Aerator with laminar flow Newest Sensor technology for better detection and operation comfort Bluetooth technology for easy adjustment to personalize settings Antiscalding protection for Sensor and Bidetta usage Support Digital Service" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Switzerland;Belgium;Netherlands;Italy" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/45252219" (IFCTEXT)
    Model = "45252219 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    Name_en = "45252219 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "45252219" (IFCTEXT)
    Product Family = "HANSACLINICA Hybrid" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/45252219" (IFCTEXT)
    Product URL = "http://static.hansa.com/45252219" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/45252219/en" (IFCTEXT)
    Type Name = "45252219 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Additional Features = "Supports Digital Service from HANSA" (IFCTEXT)
    Advanced Features = "Inner body made of DZR brass;Waterways without nickel coating;3S-installation system for safe and simple mounting;Software settings adjustable via App" (IFCTEXT)
    Aerator = "Laminar stream" (IFCTEXT)
    Afterflow Period = "3 s (1-20 s)" (IFCTEXT)
    Automatic Flush Frequency = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Electronic Parts = ";Solenoid valve;Low battery indicator" (IFCTEXT)
    Flow Rate At 300kPa = 0.000353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Single operating lever/handle;Loop shape;Hot/Cold symbols" (IFCTEXT)
    Max Flow Period = "10 s(1 - 1800 s)" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "ø 40 mm ceramic cartridge for flow and temperature control" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Pressure Loss With Flow 01ls = 300000. (IFCPRESSUREMEASURE) [PASCAL]
    Spout Projection = "115 mm" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature Adjustments = "Limitation option for maximum temperature and flow-rate" (IFCTEXT)
    Working Pressure = "50 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "45252219(2023): 45252219 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    Family and Type = "45252219(2023): 45252219 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "45252219(2023): 45252219 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    Type Id = "45252219(2023): 45252219 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "45252219(2023)" (IFCTEXT)
    Features = "Hybrid;Bluetooth®" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "45252219" (IFCTEXT)
    Name = "45252219 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "50x165x170 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Battery = "AA 1.5 V Lithium x 2" (IFCTEXT)
    Bluetooth = "5.x (D060576)" (IFCTEXT)
    Electrical Connection = "3 / 9 V" (IFCTEXT)
    Operating Voltage = 39. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "45252219(2023)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/06/2023" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4057304019647" (IFCTEXT)
    EMC Directive = "2014/53/EU , 2011/65/EU" (IFCTEXT)
    EN Standard = "EN 817, EN 15091" (IFCTEXT)
    ETIM Class Number = "EC010340 Electronic tap" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "606 x 224 x 88" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.hansa.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.hansa.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/45252219" (IFCTEXT)
    URL Declaration of SCIP = "http://static.hansa.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.hansa.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.hansa.com/doc/EcoLabel" (IFCTEXT)
    URL Materials Declaration = "http://www.hansa.com/fileadmin/resources/182718_45252219_materialsdeclaration.pdf" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL UWL = "http://static.hansa.com/UWL/45252219" (IFCTEXT)
    URL WEEE = "http://static.hansa.com/WEEE/45252219" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)