IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2022-08-22T09:29:06"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Alternate UI 18.0.0.420"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "01516283 Washbasin faucet" | object type "01516283 Washbasin faucet" | names: "01516283(2022):01516283 Washbasin faucet:13458" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "01516283 Washbasin faucet" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.137173353844829 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.00950472167011726 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    NominalDepth = 237.4 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 186.067142600916 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 214.999999999998 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/01516283" (IFCTEXT)
    3D View = "https://static.hansa.com/3D/01516283" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/01516283" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/01516283" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/01516283/en/fdv" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/01516283" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/01516283" (IFCTEXT)
    Long Marketing = "HANSACLINICA wall-mounted washbasin faucet. Firm lever offers good usability to all users and situations. Swivel spout 120° (length=150 mm) with nickel-free waterways and laminar flow. The angle of swiveling can be limited to 60° or it can be locked. In-built limitation options for water temperature and maximum flow-rate. Includes three-time sealed cover plates." (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Belgium;Netherlands;France;Czech Republic;Slovakia;Italy;Spain" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/01516283" (IFCTEXT)
    Model = "01516283 Washbasin faucet" (IFCTEXT)
    Name_en = "01516283 Washbasin faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "01516283" (IFCTEXT)
    Product Family = "HANSACLINICA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/01516283" (IFCTEXT)
    Product URL = "http://static.hansa.com/01516283" (IFCTEXT)
    Spare-Part Information URL = "http://static.hansa.com/sp/01516283" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/01516283/en" (IFCTEXT)
    Type Name = "01516283 Washbasin faucet" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Inner body made of DZR brass;Waterways without nickel coating" (IFCTEXT)
    Aerator = "Laminar stream" (IFCTEXT)
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Connection = "Eccentric coupling(s);Cover plate(s);with integrated shut-off valve(s);Silencer(s);Cover plate triple sealed" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation Width = "CC150± 15 mm" (IFCTEXT)
    Lever Handle = "Single operating lever/handle;Long shape;Hot/Cold symbols" (IFCTEXT)
    Max. Hot Water Supply = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "ø 40 mm ceramic cartridge for flow and temperature control;Litter filter(s)" (IFCTEXT)
    Mounting Holes = "2 hole" (IFCTEXT)
    Spout Projection = "227 mm" (IFCTEXT)
    Spout Swivel Range = "120° (60° / 0°)" (IFCTEXT)
    Spout Type = "Swivel spout;Swivel range limiting option" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature Adjustments = "Limitation option for maximum temperature and flow-rate ;Adjustable hot water stop (included, retrofittable)" (IFCTEXT)
    Working Pressure = "50 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "01516283(2022): 01516283 Washbasin faucet" (IFCLABEL)
    Family and Type = "01516283(2022): 01516283 Washbasin faucet" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "01516283(2022): 01516283 Washbasin faucet" (IFCLABEL)
    Type Id = "01516283(2022): 01516283 Washbasin faucet" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "01516283(2022)" (IFCTEXT)
    Features = "Single-lever" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "01516283" (IFCTEXT)
    Name = "01516283 Washbasin faucet" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "220 x 240 x 190mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "01516283(2022)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_104" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/07/2022" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4057304018909" (IFCTEXT)
    EN Standard = "EN 817" (IFCTEXT)
    ETIM Class Number = "EC011328 Washbasin mixing tap" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "278 x 218 x 202" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/01516283" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)