IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2020-07-14T18:17:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190508_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "vbu737AR" of Organization (no name given)
  Owner history of Person "vbu737AR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "4435013033 Shower system" | object type "4435013033 Shower system" | names: "4435013033(2020):4435013033 Shower system:434484" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "4435013033 Shower system" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type), Mechanical(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "4435013033(2020)" (IFCTEXT)
    Features = "Thermostatic" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "4435013033" (IFCTEXT)
    Name = "4435013033 Shower system" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "290 x 545 x 1165 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Class = "Thermostatic" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/4435013033/en/fdv" (IFCTEXT)
    Group = "Shower systems" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Model = "4435013033 Shower system" (IFCTEXT)
    Name_en = "4435013033 Shower system" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "5.39 kg" (IFCTEXT)
    Package external Dimensions = "1154 x 383 x 98" (IFCTEXT)
    Product Code = "4435013033" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/4435013033/en" (IFCTEXT)
    Product Family = "HANSAMICRA" (IFCTEXT)
    Product URL = "http://static.hansa.com/4435013033" (IFCTEXT)
    Product data url = "1" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/4435013033/en" (IFCTEXT)
    Type Name = "4435013033 Shower system" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "4435013033" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "4435013033 Shower system" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 1.13586220104517 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.185086281880994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "56" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "4435013033(2020): 4435013033 Shower system" (IFCLABEL)
    Family and Type = "4435013033(2020): 4435013033 Shower system" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "4435013033(2020): 4435013033 Shower system" (IFCLABEL)
    Type Id = "4435013033(2020): 4435013033 Shower system" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    NominalDepth = 546. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 1165. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 291. (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 445470. (IFCLENGTHMEASURE) [MILLI METRE]
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "4435013033(2020)" (IFCTEXT)
    ConvergoRefNr = "0087-2006-0066-FI" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "14/07/2020" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Approval ACS = "20 ACC LY 145" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "4057304015861" (IFCTEXT)
    EN Standard = "EN 1111" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "Can be shortened" (IFCTEXT)
    Connection = "Eccentric unions;;" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    DN Size = "DN 15" (IFCTEXT)
    Diverter = ";Integrated diverter / Volume control" (IFCTEXT)
    Flow Rate At 300kPa = 0.00918181334758703 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower Size = "Ø 95 mm" (IFCTEXT)
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation Width = "CC150± 15 mm" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/4435013033" (IFCTEXT)
    Lever Handle = "Temperature control handle;Flow control handle" (IFCTEXT)
    Max. Hot Water Supply = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part;;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Over Head Shower Size = "Ø 200 mm" (IFCTEXT)
    Pressure Loss With Flow 02ls = 180000. (IFCPRESSUREMEASURE) [PASCAL]
    Shower Parts = "Hand shower;Shower head;Shower Hose (1750 mm);Wall distance adjustable;;" (IFCTEXT)
    Shower Spray = "Regular refreshing;Relaxing soft;Sensitive" (IFCTEXT)
    Shower Spray Number = "3spray" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/4435013033" (IFCTEXT)
    Temperature Adjustments = "Thermostatic safety stop at 38°C;THERMO COOL" (IFCTEXT)