IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2023-10-21T20:07:43"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20191106_1200(x64) - Exporter 20.2.1.1 - Alternate UI 20.2.1.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1697908062 (2023-10-21T17:07:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "52682267 Washbasin faucet" | object type "52682267(2022):52682267 Washbasin faucet" | names: "52682267(2022):52682267 Washbasin faucet:449253" | material: "Brass" | property sets: Pset_DistributionFlowElementCommon, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCVALVETYPE "52682267 Washbasin faucet" | FAUCET | 1 occurrence | material: "Brass" | property sets: Constraints, Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "52682267 Washbasin faucet" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Color = "Chrome" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 1 object (1 IFCFLOWCONTROLLER)
    BarCode = "n/a" (IFCIDENTIFIER)
    SerialNumber = "n/a" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "HANSA" (IFCLABEL)
    ModelReference = "52682267" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Name = "52682267 Washbasin faucet" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "52682267 Washbasin faucet" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DistanceX-Axis = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    DistanceY-Axis = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetDefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Hand Shower Visibility = TRUE (IFCBOOLEAN)
    HandShowerDefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0815960318768056 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00224524250859163 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    FaucetNominalDepth = 148.345730833423 (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalHeight = 188.503678912302 (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalWidth = 46.4999051570868 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalDepth = 64.3 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalHeight = 296.7 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalWidth = 49.3 (IFCLENGTHMEASURE) [MILLI METRE]
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "32" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/52682267" (IFCTEXT)
    3D View = "https://static.hansa.com/AR/52682267" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/52682267" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/52682267" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/52682267/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/52682267" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/52682267" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/52682267" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Belgium;Netherlands;Czech Republic;Slovakia;Italy" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/52682267" (IFCTEXT)
    Model = "52682267 Washbasin faucet" (IFCTEXT)
    Name_en = "52682267 Washbasin faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "52682267" (IFCTEXT)
    Product Family = "HANSAVANTIS XL" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/52682267" (IFCTEXT)
    Product URL = "http://static.hansa.com/52682267" (IFCTEXT)
    Spare-Part Information URL = "http://static.hansa.com/sp/52682267" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/52682267/en" (IFCTEXT)
    Type Name = "52682267 Washbasin faucet" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Inner body made of DZR brass;3S-installation system for safe and simple mounting" (IFCTEXT)
    Aerator = "PCA® - constant flow rate regardless of pressure variations" (IFCTEXT)
    Backflow Prevention EN1717 = "HC" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Excluded Items = "Without pop-up waste" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.000353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower = "Bidetta hand shower" (IFCTEXT)
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Single operating lever/handle;Pin shape;Hot/Cold symbols" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "30Cartridge" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Shower Parts = "Hand shower;Shower holder" (IFCTEXT)
    Spout Projection = "114 mm" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature = "" (IFCTEXT)
    Temperature Adjustments = "Limitation option for maximum temperature and flow-rate" (IFCTEXT)
    Working Pressure = "50 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "52682267(2022): 52682267 Washbasin faucet" (IFCLABEL)
    Family and Type = "52682267(2022): 52682267 Washbasin faucet" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "52682267(2022): 52682267 Washbasin faucet" (IFCLABEL)
    Type Id = "52682267(2022): 52682267 Washbasin faucet" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "52682267(2022)" (IFCTEXT)
    Features = "Single-lever;Bidetta" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "52682267" (IFCTEXT)
    Name = "52682267 Washbasin faucet" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "Faucet:45x150x190 mm / Hand shower:50x65x295 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBLProjectId = "5d1062b1-121a-4f1f-a2d7-5f519d3e89c8" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "52682267(2022)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/06/2023" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Green Building Properties | properties | on 1 type object
    CO2 Emissions (A1-A3) = 10.51 (IFCREAL)
    CO2 Emissions (A4) = 0.29 (IFCREAL)
    CO2 Emissions (B7) = 1854. (IFCREAL)
    CO2 Emissions (C2) = 0.02 (IFCREAL)
    CO2 Emissions (C3) = 0.02 (IFCREAL)
    CO2 Emissions (C4) = 0.08 (IFCREAL)
    CO2 Emissions (D) = -7.47 (IFCREAL)
    EAN Number = "4057304017247" (IFCTEXT)
    EN Standard = "EN 817" (IFCTEXT)
    ETIM Class Number = "EC011328 Washbasin mixing tap" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "754 x 334 x 63" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.hansa.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.hansa.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/52682267" (IFCTEXT)
    URL Declaration of SCIP = "http://static.hansa.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.hansa.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.hansa.com/doc/EcoLabel" (IFCTEXT)
    URL Environmental Product Declaration EPD = "http://www.hansa.com/fileadmin/resources/184523_EPD_Washbasin faucet.pdf" (IFCTEXT)
    URL Materials Declaration = "http://www.hansa.com/fileadmin/resources/168482_52682267_materialsdeclaration.pdf" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL UWL = "http://static.hansa.com/UWL/52682267" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Pset_ValveTypeCommon | properties | on 1 type object
    CloseOffRating = 0. (IFCPRESSUREMEASURE) [PASCAL]
    FlowCoefficient = 0. (IFCREAL)
    ValveMechanism in {"n/a"} (IFCLABEL)
    ValveOperation in {"n/a"} (IFCLABEL)
    ValvePattern in {"n/a"} (IFCLABEL)
  Pset_ValveTypeFaucet | properties | on 1 type object
    Finish = "Polished" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"