IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2021-03-01T13:58:02"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Alternate UI 18.0.0.420"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "cjl@convergo.se" of Organization (no name given)
  Owner history of Person "cjl@convergo.se" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "00870019 Washbasin faucet, 3 V, Bluetooth" | object type "00870019 Washbasin faucet, 3 V, Bluetooth" | names: "00870019(2020):00870019 Washbasin faucet, 3 V, Bluetooth:350759" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "00870019 Washbasin faucet, 3 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, Electrical, Electrical Engineering, General, Green Building Properties, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0389244337650137 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 20. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.00120152380853874 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    NominalDepth = 214.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 74.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 74.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 175. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/00870019" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/00870019" (IFCTEXT)
    Class = "Touchless;Battery-operated;Bluetooth®" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/00870019" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/00870019/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/00870019" (IFCTEXT)
    Group = "Washbasin faucets" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Market = "AUT;BEL;CZE;DEU;ESP;FRA;INT;ITA;NLD;SVK" (IFCTEXT)
    Model = "Name_en" (IFCTEXT)
    Name_en = "00870019 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "1.355 kg" (IFCTEXT)
    Package external Dimensions = "240 x 85 x 66" (IFCTEXT)
    Product Code = "00870019" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/00870019/en" (IFCTEXT)
    Product Family = "HANSAELECTRA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/00870019" (IFCTEXT)
    Product URL = "http://static.hansa.com/00870019" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/00870019/en" (IFCTEXT)
    Type Name = "00870019 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Adjustable settings (via bluetooth)" (IFCTEXT)
    Aerator = "Pressure controlled aerator;Laminar;Burglarproof" (IFCTEXT)
    Afterflow Period = 3120. (IFCREAL)
    Automatic Flush = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    DN Size = "DN15" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.000353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/00870019" (IFCTEXT)
    Max Flow Period = 211800. (IFCREAL)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Noise Class = "I (ISO 3822) Oras lab." (IFCTEXT)
    Protection Class = "IP 55" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/00870019" (IFCTEXT)
    Spout Type = "Fixed spout;" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "00870019(2020): 00870019 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    Family and Type = "00870019(2020): 00870019 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "00870019(2020): 00870019 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    Type Id = "00870019(2020): 00870019 Washbasin faucet, 3 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Public & Semi-public" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "00870019(2020)" (IFCTEXT)
    Features = "Touchless;Battery-operated;Bluetooth®" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "00870019" (IFCTEXT)
    Name = "00870019 Washbasin faucet, 3 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "75x215x75 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Electrical | properties | on 1 type object
    Battery = "AA 1.5 V Lithium x 2" (IFCTEXT)
    Operating Voltage = 3. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Electrical Engineering | properties | on 1 type object
    Bluetooth = "4.x" (IFCTEXT)
    Electronic Parts = "Autofocus sensor;Solenoid valve;Low battery indication" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "00870019(2020)" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_81" (IFCTEXT)
    Uniclass2015Description = "Shower thermostatic water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_81" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "16/02/2021" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Customs Code = "84818019" (IFCTEXT)
    EAN Number = "4057304015885" (IFCTEXT)
    EMC Directive = "2014/30/EU" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)