IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2019-03-15T13:57:08"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.6.0.0 - Alternate UI 16.6.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "davidbrb22DR27U" of Organization (no name given)
  Owner history of Person "davidbrb22DR27U" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "08302281 Washbasin faucet" | object type "08302281 Washbasin faucet" | names: "08302281:08302281 Washbasin faucet:315415" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "08302281 Washbasin faucet" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type), Mechanical(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Health care" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "08302281" (IFCTEXT)
    Features = "Thermostatic" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "08302281" (IFCTEXT)
    Name = "08302281 Washbasin faucet" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "282x194x140 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/08302281" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/08302281" (IFCTEXT)
    Class = "Thermostatic" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/08302281" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/08302281/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/08302281" (IFCTEXT)
    Group = "Washbasin faucets" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Market = "INT;DNK;EST;FIN;LVA;LTU;POL;RUS;SWE;UKR" (IFCTEXT)
    Model = "08302281 Washbasin faucet" (IFCTEXT)
    Name_en = "08302281 Washbasin faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "n/a" (IFCTEXT)
    Package external Dimensions = "430 x 215 x 191" (IFCTEXT)
    Product Code = "08302281" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/08302281/en" (IFCTEXT)
    Product Family = "HANSACARE" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/08302281" (IFCTEXT)
    Product URL = "http://static.hansa.com/08302281" (IFCTEXT)
    Type Name = "08302281 Washbasin faucet" (IFCTEXT)
    URL = "" (IFCTEXT)
    Usage Group = "Health centers & Child welfare clinics;Hospitals" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "08302281" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "08302281 Washbasin faucet" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.123009080931488 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.0076341209306585 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "15" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "08302281: 08302281 Washbasin faucet" (IFCLABEL)
    Family and Type = "08302281: 08302281 Washbasin faucet" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "08302281: 08302281 Washbasin faucet" (IFCLABEL)
    Type Id = "08302281: 08302281 Washbasin faucet" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    NominalWidth = 282. (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 179. (IFCLENGTHMEASURE) [MILLI METRE]
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "08302281" (IFCTEXT)
    ConvergoRefNr = "0087-1803-0006-FI" (IFCTEXT)
    ManufacterURL = "http://www.hansa.com/" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basin and troughs" (IFCTEXT)
    NBSReference = "45-35-70/370" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "12/03/2019" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Approval ABP = "PA-IX 28551/IA" (IFCTEXT)
    Approval DVGW = "NW-6509CR0103" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "4057304013393" (IFCTEXT)
    EN Standard = "EN 1111" (IFCTEXT)
    URL ABP = "http://static.hansa.com/ABP/08302281" (IFCTEXT)
    URL DVGW = "http://static.hansa.com/DVGW/08302281" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "DZR brass;;Thermal disinfection according to DVGW W 551" (IFCTEXT)
    Aerator = "Care® flow straightener;Laminar" (IFCTEXT)
    Connection = "Covered eccentric unions" (IFCTEXT)
    DN Size = "DN15" (IFCTEXT)
    Flow Rate At 300kPa = 0.00706293334429772 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Wall-mounted" (IFCTEXT)
    Installation Width = "cc150 ± 10 mm" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/08302281" (IFCTEXT)
    Lever Handle = "Flow control handle" (IFCTEXT)
    Max. Hot Water Supply = 90. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part;Litter filter(s);Shut-off valve" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/08302281" (IFCTEXT)
    Spout Swivel Range = "120°" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Temperature = "THERMO COOL;Temperature limiter;Thermostatic temperature control;Thermostatic safety stop at 38°C" (IFCTEXT)
  Text(Type) | properties | on 1 type object
    Health Sales Arguments = "Thermostat is suitable for thermal disinfection, which is particularly important for public or large-scale facilities." (IFCTEXT)
    Safety Sales Arguments = "THERMO COOL. Improved safety – the housing of the fittings conducts minimal heat." (IFCTEXT)
    Technology Sales Arguments = "Suitable for instantaneous water heaters (shower above 20 kW or bathtub" (IFCTEXT)