IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2022-08-23T00:58:40"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Alternate UI 18.0.0.420"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCSANITARYTERMINALTYPE "44290180 Overhead shower, d 95 mm" | object type "44290180 Overhead shower, d 95 mm" | names: "44290180(2022):44290180 Overhead shower, d 95 mm:354558" | property sets: Constraints, Dimensions, Identity Data, Other, Phasing

Types
  IFCSANITARYTERMINALTYPE "44290180 Overhead shower, d 95 mm" | SHOWER | 1 occurrence | property sets: Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes, Mechanical

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWTERMINAL)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWTERMINAL)
    Area = 0.0196946676349944 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.000506748616587175 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    NominalDepth = 95.0276014444034 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 56.1300374123078 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 95.0164105608465 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWTERMINAL)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/44290180" (IFCTEXT)
    3D View = "https://static.hansa.com/3D/44290180" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/44290180" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Collection = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/44290180" (IFCTEXT)
    EANNumber = "" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/44290180/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/44290180" (IFCTEXT)
    Group = "Overhead shower" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/44290180" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/44290180" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Belgium;Netherlands;France;Czech Republic;Slovakia;Italy;Spain" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/44290180" (IFCTEXT)
    Model = "44290180 Overhead shower, d 95 mm" (IFCTEXT)
    Name_en = "44290180 Overhead shower, d 95 mm" (IFCTEXT)
    OmniClass Number = "23.45.05.14.17" (IFCTEXT)
    OmniClass Title = "Showers" (IFCTEXT)
    Product Code = "44290180" (IFCTEXT)
    Product Family = "HANSAMEDIJET" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/44290180" (IFCTEXT)
    Product URL = "http://static.hansa.com/44290180" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/44290180/en" (IFCTEXT)
    Type Name = "44290180 Overhead shower, d 95 mm" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "44290180(2022): 44290180 Overhead shower, d 95 mm" (IFCLABEL)
    Family and Type = "44290180(2022): 44290180 Overhead shower, d 95 mm" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "44290180(2022): 44290180 Overhead shower, d 95 mm" (IFCLABEL)
    Type Id = "44290180(2022): 44290180 Overhead shower, d 95 mm" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "n/a" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Years" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "44290180(2022)" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "n/a" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "44290180" (IFCTEXT)
    Name = "44290180 Overhead shower, d 95 mm" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "95 x 95 x 60 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Years" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWTERMINAL)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "44290180(2022)" (IFCTEXT)
    ExpiringDate = "n/a" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Shower heads" (IFCTEXT)
    NBSReference = "45-35-70/333" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_76" (IFCTEXT)
    Uniclass2015Description = "Shower heads" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_76" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "18/08/2022" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4057304018572" (IFCTEXT)
    ETIM Class Number = "EC011383 Shower head" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "96 x 96 x 58" (IFCTEXT)
    UNSPSC Class Number = "30181801 Shower head" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    ShowerSetMainMaterial = "Brass" (IFCLABEL)
  Mechanical | properties | on 1 type object
    Connection Size = "G1/2" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.00706293334429772 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower Size = "Ø 95mm" (IFCTEXT)
    Max. Hot Water Supply = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Shower Parts = "Rotatable ball joint connection;Anti limescale technology (easy to clean)" (IFCTEXT)
    Shower Spray = "Low aerosol" (IFCTEXT)
    Shower Spray Number = "1 shower spray" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Working Pressure = "50 - 1000 kPa" (IFCTEXT)