IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2019-09-06T12:51:05"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190508_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "cjl@convergo.se" of Organization (no name given)
  Owner history of Person "cjl@convergo.se" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 1566398227 (2019-08-21T14:37:07Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "44770111 Shower set" | object type "44770111 Shower set" | names: "44770111:44770111 Shower set:501850" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Other

Types
  IFCVALVETYPE "44770111 Shower set" | FAUCET | 1 occurrence | property sets: Dimensions(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type), Mechanical(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "44770111" (IFCTEXT)
    Features = "n/a" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "44770111" (IFCTEXT)
    Name = "44770111 Shower set" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "220x130x760 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/44770111" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/44770111" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/44770111" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/44770111/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/44770111" (IFCTEXT)
    Group = "Hand showers and shower sets" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Model = "44770111 Shower set" (IFCTEXT)
    Name_en = "44770111 Shower set" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "1.125 kg" (IFCTEXT)
    Package external Dimensions = "781 x 156 x 55" (IFCTEXT)
    Product Code = "44770111" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/44770111/en" (IFCTEXT)
    Product Family = "HANSABASICJET Style" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/44770111" (IFCTEXT)
    Product URL = "http://static.hansa.com/44770111" (IFCTEXT)
    Type Name = "44770111 Shower set" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "44770111" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "44770111 Shower set" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.295348900069314 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.0218004830430762 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "44770111: 44770111 Shower set" (IFCLABEL)
    Family and Type = "44770111: 44770111 Shower set" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "44770111: 44770111 Shower set" (IFCLABEL)
    Type Id = "44770111: 44770111 Shower set" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBLProjectId = "8b2fe5c3-633f-4129-b12a-2a6d73f37baa" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    NominalDepth = 129.564240647513 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 760. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 221.2 (IFCLENGTHMEASURE) [MILLI METRE]
    Pipe Length = 720. (IFCLENGTHMEASURE) [MILLI METRE]
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "44770111" (IFCTEXT)
    ConvergoRefNr = "0087-1909-0121-FI" (IFCTEXT)
    ManufacterURL = "http://www.hansa.com/" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "25/07/2019" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Customs Code = "39249000" (IFCTEXT)
    EAN Number = "4057304011078" (IFCTEXT)
    EN Standard = "EN 1112" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Connection Size = "G1/2" (IFCTEXT)
    Flow Rate At 300kPa = 0.0105944000164466 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower Size = "96 mm" (IFCTEXT)
    Installation Type = "Wall-mounted" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/44770111" (IFCTEXT)
    Max. Hot Water Supply = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]