IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2022-05-19T15:39:04"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.4.0.0 - Alternate UI 18.4.0.0"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "54652209 Washbasin faucet, 230/9 V, Bluetooth" | object type "54652209(2022):54652209 Washbasin faucet, 230/9 V, Bluetooth" | names: "54652209(2022):54652209 Washbasin faucet, 230/9 V, Bluetooth:297080" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "54652209 Washbasin faucet, 230/9 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, Electrical Engineering, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "54652209(2022): 54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    Family and Type = "54652209(2022): 54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "54652209(2022): 54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    Type Id = "54652209(2022): 54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "54652209(2022)" (IFCTEXT)
    Features = "Single-lever, side operated;Hybrid;Plug transformer;Bluetooth®" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "54652209" (IFCTEXT)
    Name = "54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "55x175x165 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/54652209" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/54652209" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/54652209" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/54652209/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/54652209" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/54652209" (IFCTEXT)
    Item Type = "Sales item" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Belgium;Netherlands;France;Czech Republic;Slovakia;Italy;Spain" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/54652209" (IFCTEXT)
    Model = "54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    Name_en = "54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "54652209" (IFCTEXT)
    Product Family = "HANSAVANTIS Style" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/54652209" (IFCTEXT)
    Product URL = "http://static.hansa.com/54652209" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/54652209/en" (IFCTEXT)
    Type Name = "54652209 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0867111555203857 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00433945211896124 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Inner body made of DZR brass" (IFCTEXT)
    Aerator = "Standard aerator;PCA® - constant flow rate regardless of pressure variations" (IFCTEXT)
    Automatic Flush Frequency = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Electronic Parts = "Infrared sensor;Solenoid valve;Power supply;Low battery indicator" (IFCTEXT)
    Excluded Items = "Without pop-up waste" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.000353146667214886 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Single operating lever/handle;Hot/Cold symbols" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "30Cartridge" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Spout Projection = "147 mm" (IFCTEXT)
    Spout Swivel Range = "120°" (IFCTEXT)
    Spout Type = "Swivel spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature = "Temperature limiter" (IFCTEXT)
    Temperature Adjustments = "Limitation option for maximum temperature and flow-rate ;Adjustable hot water stop (included, retrofittable)" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "Phase 1" (IFCLABEL)
  Electrical Engineering | properties | on 1 type object
    Bluetooth = "5.x" (IFCTEXT)
    Electrical Connection = "230 / 9 V" (IFCTEXT)
    Operating Voltage = 9. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMstone" (IFCTEXT)
    BIMObjectName = "54652209(2022)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_78" (IFCTEXT)
    Uniclass2015Description = "Shower manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_78" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "17/05/2022" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    EAN Number = "4057304017513" (IFCTEXT)
    EMC Directive = "2014/53/EU , 2011/65/EU" (IFCTEXT)
    EN Standard = "EN 817, EN 15091" (IFCTEXT)
    ETIM Class Number = "EC011328 Washbasin mixing tap" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/54652209" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL WEEE = "http://static.hansa.com/WEEE/54652209" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"