IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2022-08-22T09:25:20"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170223_1515(x64) - Exporter 18.0.0.420 - Alternate UI 18.0.0.420"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "64162219 Washbasin faucet, 6 V, Bluetooth" | object type "64162219 Washbasin faucet, 6 V, Bluetooth" | names: "64162219:64162219 Washbasin faucet, 6 V, Bluetooth:4532" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "64162219 Washbasin faucet, 6 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, Electrical Engineering, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0396551751230666 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00131774053782049 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 155.223165740614 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 127.600000000001 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 66.2928819806354 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/64162219" (IFCTEXT)
    3D View = "https://static.hansa.com/3D/64162219" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/64162219" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/64162219" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/64162219/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/64162219" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/64162219" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/64162219" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/64162219" (IFCTEXT)
    Model = "64162219 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    Name_en = "64162219 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "64162219" (IFCTEXT)
    Product Family = "HANSAELECTRA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/64162219" (IFCTEXT)
    Product URL = "http://static.hansa.com/64162219" (IFCTEXT)
    Spare-Part Information URL = "http://static.hansa.com/sp/64162219" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/64162219/en" (IFCTEXT)
    Type Name = "64162219 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Software settings adjustable via App" (IFCTEXT)
    Aerator = "Hidden aerator;PCA® - constant flow rate regardless of pressure variations" (IFCTEXT)
    Afterflow Period = "3 s (1-20 s)" (IFCTEXT)
    Automatic Flush Frequency = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Electronic Parts = "Autofocus infrared sensor;Solenoid valve;Low battery indicator" (IFCTEXT)
    Extensions = "Push pop-up waste without draw-rod" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.00317832000493397 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Temperature control handle" (IFCTEXT)
    Max Flow Period = "2 min (1 - 1800 s)" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Mixing valve for manual temperature control;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Operating Distance = "20-130 mm (110/130/160 mm)" (IFCTEXT)
    Spout Projection = "110 mm" (IFCTEXT)
    Spout Type = "Fixed spout;Casted construction" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature = "Temperature limiter (retrofittable)" (IFCTEXT)
    Temperature Adjustments = "Adjustable hot water stop (included, retrofittable)" (IFCTEXT)
    Working Pressure = "50 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "64162219: 64162219 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    Family and Type = "64162219: 64162219 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "64162219: 64162219 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    Type Id = "64162219: 64162219 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "Single lever" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "64162219" (IFCTEXT)
    Features = "Touchless;Battery-operated;Bluetooth®" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "64162219" (IFCTEXT)
    Name = "64162219 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "65x155x130 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical Engineering | properties | on 1 type object
    Battery = "Lithium 2CR5 6 V" (IFCTEXT)
    Bluetooth = "4.x (D034445)" (IFCTEXT)
    Operating Voltage = 6. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "64162219" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "3" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "3" (IFCTEXT)
    VersionDate = "01/07/2022" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    Approval DVGW = "CW-6514CR0161" (IFCTEXT)
    EAN Number = "4057304018947" (IFCTEXT)
    EMC Directive = "2014/53/EU , 2011/65/EU" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
    ETIM Class Number = "EC010340 Electronic tap" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "290 x 210 x 90" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL DVGW = "http://static.hansa.com/DVGW/64162219" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/64162219" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL UN38.3 = "http://www.hansa.com/fileadmin/resources/163480_UN38-3_Maxell_2CR5_198330-77.pdf3.pdf" (IFCTEXT)
    URL WEEE = "http://www.hansa.com/fileadmin/resources/153036_WEEE.pdf" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)