IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2022-03-21T14:03:28"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190510_1515(x64) - Exporter 18.3.3.18 - Alternate UI 18.3.3.18"
Application: "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)"

People and organizations
  Person "cjl@convergo.se" of Organization (no name given)
  Owner history of Person "cjl@convergo.se" of Organization (no name given) | application "Autodesk Revit 2018 (ENU)" version "2018" identifier "Revit" by Organization "Autodesk Revit 2018 (ENU)" | change NOCHANGE | created 1566398227 (2019-08-21T14:37:07Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "65242213 Kitchen faucet with dishwasher valve, 230/5 V" | object type "65242213 Kitchen faucet with dishwasher valve, 230/5 V" | names: "65242213:65242213 Kitchen faucet with dishwasher valve, 230/5 V:493549" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "65242213 Kitchen faucet with dishwasher valve, 230/5 V" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, Electrical Engineering, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "HANSA" (IFCLABEL)
    ModelReference = "65242213" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.143066786426732 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00915340066531412 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 255.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 293.500000000002 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 122. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/65242213" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/65242213" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/65242213" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/65242213/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/65242213" (IFCTEXT)
    Group = "Kitchen faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.hansa.com/manual/65242213" (IFCTEXT)
    Interactive AR View URL = "https://static.hansa.com/AR/65242213" (IFCTEXT)
    Item Type = "Sales item" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "Austria;Belgium;Czech Republic;Germany;Spain;France;International;Italy;Netherlands;Slovakia" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/65242213" (IFCTEXT)
    Model = "65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCTEXT)
    Name_en = "65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "65242213" (IFCTEXT)
    Product Family = "HANSAFIT" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/65242213" (IFCTEXT)
    Product URL = "http://static.hansa.com/65242213" (IFCTEXT)
    Spare-Part Information URL = "http://static.hansa.com/sp/65242213" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/65242213/en" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Additional Features = "Faucet is GGT-approved user test VERY GOOD" (IFCTEXT)
    Advanced Features = "Surfaces in contact with drinking water contain less than 0.3% lead;Inner body made of DZR brass;Waterways without nickel coating;Software settings adjustable via buttons" (IFCTEXT)
    Aerator = "Hidden aerator;Standard aerator" (IFCTEXT)
    Afterflow Period = "4 s (2/4/8/10/20 s)" (IFCTEXT)
    Automatic Flush Frequency = "off (off/12/24/48/72 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (10/30/60/120/180 s)" (IFCTEXT)
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Dishwasher Valve = "Electronic stop valve for external equipment" (IFCTEXT)
    Dishwasher Valve Open Period = "4 h / 12 h" (IFCTEXT)
    Electronic Parts = "Autofocus infrared sensor;Solenoid valve;External control unit;Power supply;Light indicated function(s)" (IFCTEXT)
    Flow Rate At 300kPa = 0.00706293334429772 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Two operating levers/handles;Easy-Grip surface" (IFCTEXT)
    Max Flow Period = "40 s (10/40/60/120/180 s)" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part for flow control;Mixing valve for manual temperature control;Litter filter(s)" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Operating Distance = "0-40 mm" (IFCTEXT)
    Pressure Loss With Flow 02ls = 290000. (IFCPRESSUREMEASURE) [PASCAL]
    Spout Projection = "193 mm" (IFCTEXT)
    Spout Swivel Range = "120° (80° / 60°)" (IFCTEXT)
    Spout Type = "Swivel spout;Swivel range limiting option" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "65242213: 65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCLABEL)
    Family and Type = "65242213: 65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "65242213: 65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCLABEL)
    Type Id = "65242213: 65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Kitchen" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "65242213" (IFCTEXT)
    Features = "Hybrid;Plug transformer;Dishwasher valve" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "brassPlastic" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "65242213" (IFCTEXT)
    Name = "65242213 Kitchen faucet with dishwasher valve, 230/5 V" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "120x255x300 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBLProjectId = "8b2fe5c3-633f-4129-b12a-2a6d73f37baa" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "65242213" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "18/03/2022" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Electrical Engineering | properties | on 1 type object
    Electrical Connection = "230 / 5 V" (IFCTEXT)
    Operating Voltage = 5. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 54 / transformer IP 20" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4015474273450" (IFCTEXT)
    EMC Directive = "2014/30/EU , 2014/35/EU , 2011/65/EU" (IFCTEXT)
    EN Standard = "EN 1111" (IFCTEXT)
    ETIM Class Number = "EC011431 Kitchen mixing tap" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "460 x 300 x 130" (IFCTEXT)
    Sales Package gross weight = "3.87 kg" (IFCTEXT)
    Sales Package package weight = "0.6062 kg" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/65242213" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL WEEE = "http://static.hansa.com/WEEE/65242213" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)